Assessment Requirements for CPCCWHS1001 Prepare to work safely in the construction industry

Release: 1

Assessment Requirements for CPCCWHS1001 Prepare to work safely in the construction industry

Modification History

Release	Comment
Version 1	Replaces superseded equivalent CPCCOHS1001A Work safely in the construction industry.

Performance Evidence

A person demonstrating competency in this unit must satisfy the requirements of the elements, performance criteria, foundation skills, and range of conditions of this unit, in addition to the specific performance and knowledge evidence described below.

The person must:

identify and orally report two construction hazards

orally explain how risk could be reduced or removed in relation to those two hazards

select appropriate personal protective equipment (PPE) to control the risk

orally explain basic procedures for responding to incidents and emergencies, including types and purpose of the following fire safety equipment:

fire blankets

fire extinguishers, including water, carbon dioxide, powder and foam

hose reels and mains

identify and orally explain the meaning of required safety signs and symbols

orally explain the purpose of job safety analyses (JSAs), safe work method statements (SWMS) and safety data sheets (SDS)

orally explain the roles of the following designated health and safety personnel:

first aid officers

work health and safety representatives

work health and safety committee members

supervisors.

The person must also demonstrate correctly fitting to themselves the PPE listed below:

eye protection

hearing protection

hard hat

high visibility retro reflective vest.

Knowledge Evidence

A person must demonstrate knowledge of:

basic duty of care, and the roles, rights and responsibilities of business owners and workers in relation to working safely while undertaking construction work

basic meaning of the terms ‘hazard’ and ‘risk’

basic principles of risk management, including the following five steps in order:

identify hazard

assess risk

consult and report

control hazard

review

basic procedures for accessing first aid

construction hazards, including those relating to:

asbestos

confined spaces

electrical: power lines, cords and equipment

excavations and trenches, including underground services

dust

falling objects

hazardous substances and dangerous goods

hot and cold work environments

manual handling

noise

plant and equipment operation

traffic and mobile plant

unplanned collapse

ultraviolet radiation

working at heights, including scaffolding

construction work that requires a high risk work licence

types, purpose and use of PPE used in construction, as specified in the performance evidence, and including safety footwear, harnesses and respiratory protection, and ultraviolet (UV) protective clothing and sunscreen

construction emergencies, including:

chemical spill

fire

injury to personnel

structural collapse

toxic or flammable vapour emission

vehicle or mobile plant accident

construction incidents, including:

incidents resulting in personal injury or damage to property

near misses or dangerous occurrences that do not cause injury but may pose an immediate and significant risk to persons or property, and need to be reported so that action can be taken to prevent recurrence

safe work practices that should be followed in construction work, including:

accessing and using site amenities for drinking water, hand washing and toilets

following safety procedures when performing work tasks and using equipment

identifying and reporting hazards, incidents and injuries in the workplace

keeping the work area clean, tidy and free from debris

not using or being affected by drugs and/or alcohol while at work

preventing bullying and harassment in the workplace

selecting and using required PPE

smoking only in designated areas

storing and removing waste and debris in designated areas

meanings and symbols associated with construction safety signs, symbols and tags, including:

emergency information signs: exits, emergency equipment and first aid

fire signs: location of fire alarms and firefighting equipment

hazard signs and symbols: danger and warning

regulatory signs and symbols: prohibition, mandatory and limitation or restriction

safety and lockout tags: danger and out-of-service tags.

Assessment Conditions

The following must be present and available to learners during assessment activities:

equipment:

all of the PPE listed in the performance evidence

specifications:

state or territory Act relevant to the location of the learner, as specified in the range of conditions.

The assessment of performance evidence must be done by direct observation of the learner by an assessor, either by an assessor observing the learner physically and/or by an assessor observing the learner via audio and visual media in real time.

Assessor requirements

As a minimum, assessors must satisfy the assessor requirements in the Standards for Registered Training Organisations (RTOs) current at the time of assessment.

Assessors must hold the unit CPCCOHS2001A Apply OHS requirements, policies and procedures in the construction industry, or its successor.

Links

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=7e15fa6a-68b8-4097-b099-030a5569b1ad