Assessment Requirements for AURVTT006 Apply trimming adhesives

Release: 1

Assessment Requirements for AURVTT006 Apply trimming adhesives

Modification History

Release	Comment
Release 1	New unit of competency.

Performance Evidence

Before competency can be determined, individuals must demonstrate they can perform the following according to the standard defined in this unit’s elements, performance criteria, range of conditions and foundation skills:

apply trim adhesives to three different vehicle or vessel components, in which the work must involve:

one vehicle or marine fixed cover

one vehicle or marine carpet section.

Knowledge Evidence

Individuals must be able to demonstrate knowledge of:

work health and safety (WHS) and occupational health and safety (OHS) requirements relating to applying trimming adhesives, including procedures for:

selecting and using personal protective equipment (PPE)

using specialist tools and equipment

using safety data sheets (SDS) for adhesives

handling and storing adhesives

environmental requirements, including procedures for storing and disposing of waste adhesives

types and uses of specialist trimming tools and equipment

adhesive types required for different materials, including:

polyvinyl chloride (PVC)

fabric

leather

adhesive application techniques, including:

surface preparation

application

cleaning

procedures for protecting vehicle and components when applying trim adhesives.

Assessment Conditions

Assessors must satisfy NVR/AQTF assessor requirements.

Competency is to be assessed in the workplace or a simulated environment that accurately reflects performance in a real workplace setting.

Assessment must include direct observation of tasks.

Where assessment of competency includes third-party evidence, individuals must provide evidence that links them to the vehicles where they have applied trim adhesives, e.g. work orders.

Assessors must verify performance evidence through questioning on skills and knowledge to ensure correct interpretation and application.

The following resources must be made available:

automotive or marine trimming workplace or simulated workplace

workplace instructions

SDS for adhesives

PPE required to apply trim adhesives

adhesives for PVC, fabric and leather

PVC, fabric and leather materials

three different vehicles or vessels with components requiring trimming

tools, equipment and materials appropriate for applying trim, materials and adhesives.

Links

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=b4278d82-d487-4070-a8c4-78045ec695b1

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=b4278d82-d487-4070-a8c4-78045ec695b1